### Setting of External Device

Open the channel configuration dialog box from the ladder software and set in the [Chan.0] tab as below. Please refer to the manual of the External Device for more details.

Setup Items | Setup Description
--- | ---
Driver | DH485
Baud | 19200
Max. Node Address | 31
Token Hold Factor | 1
Node Address | 1

NOTE

- There are also such cases that above settings are performed in the [Chan.1] tab depending on the connecting port.