### 1A

1:1

n:1

No. | Name | Notes
--- | --- | ---
(1) | CANopen recommended cable • Connector Display (PFXZCDEUCA1) side (slave): D-sub 9 pin (socket) Display or other slave side: Terminal block/D-sub 9 pin (socket) External Device side (master): Terminal block/D-sub 9 pin (socket) | Connect the shield to FG (Shell).

IMPORTANT:

- Be sure to connect terminal resistors (120Ω 1/4W) at both ends of the cabling connections as shown above.