# Read Format

## SIO Convert Mode

##### Command data block (from Host)

Setting range

Address: 0000H to 270FH (0 to 9999)

Number of data packets: 0001H to 0100H (1 to 256)

Be sure to make all data entries in ASCII code format.

##### Response data block (from Display)

- When there is no error

<Setting range>

Data: 0000H to FFFFH

- If an error occurs

NAK response

## SIO Extend Mode, ASCII

##### Command data block (from Host)

Marked area with asterisk (*) may not be added depending on the setting.

<Setting range>

Address: 0000H to 270FH (0 to 9999)

Number of data packets: 0001H to 0100H (1 to 256)

Be sure to make all data entries in ASCII code format.

##### Response data block (from Display)

- When there is no error

Marked area with asterisk (*) may not be added depending on the setting.

<Setting range>

Data: 0000H to FFFFH

- If an error occurs

NAK response

## SIO Extend Mode, Binary

##### Command data block (from Host)

Marked area with asterisk (*) may not be added depending on the setting.

<Setting range>

Address: 0000H to 270FH (0 to 9999)

Number of data packets: 0001H to 0200H (1 to 512)

##### Response data block (from Display)

- When there is no error

Marked area with asterisk (*) may not be added depending on the setting.

<Setting range>

Data: 0000H to FFFFH

- If an error occurs

NAK response

<Example>

The host reads hexadecimal data of 2 words in length from addresses 100 and 101 in the Memory Link.

## Convert Mode

## Extend Mode, 1:1 ASCII,

ETX. SUMCHECK: ENABLED, TERMINATOR: CR.LF, ACK: ENABLED, NAK: ENABLED

## Extend Mode, 1:n ASCII,

ETX. SUMCHECK: ENABLED, TERMINATOR: CR.LF, ACK: ENABLED, NAK: ENABLED

## Extend Mode, 1:1 BINARY,

ETX. SUMCHECK: ENABLED, ACK: ENABLED, NAK: ENABLED

## Extend Mode, 1:n BINARY,

ETX. SUMCHECK: ENABLED, ACK: ENABLED, NAK: ENABLED