### MELSEC Q (High performance model) Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Input Relay | X0000 - X1FFF | X0000 - X1FF0 |  |
Output Relay | Y0000 - Y1FFF | Y0000 - Y1FF0 |
Internal Relay | M00000 - M32767 | M00000 - M32752 |
Special Relay | SM0000 - SM2047 | SM0000 - SM2032 |
Latch Relay | L00000 - L32767 | L00000 - L32752 |
Annunciator | F00000 - F32767 | F00000 - F32752 |
Edge Relay | V00000 - V32767 | V00000 - V32752 |
Step Relay | S0000 - S8191 | S0000 - S8176 |
Link Relay | B0000 - B7FFF | B0000 - B7FF0 |
Special Link Relay | SB000 - SB7FF | SB000 - SB7F0 |
Timer (Contact) | TS00000 - TS23087 | ------ |
Timer (Coil) | TC00000 - TC23087 | ------ |
Retentive Timer (Contact) | SS00000 - SS23087 | ------ |
Retentive Timer (Coil) | SC00000 - SC23087 | ------ |
Counter (Contact) | CS00000 - CS23087 | ------ |  |
Counter (Coil) | CC00000 - CC23087 | ------ |
Timer (Current Value) | ------ | TN00000 - TN23087 |
Retentive Timer (Current Value) | ------ | SN00000 - SN23087 |
Counter (Current Value) | ------ | CN00000 - CN23087 |
Data Register | ------ | D00000 - D25983 | *1
Special Register | ------ | SD0000 - SD2047 |
Link Register | ------ | W0000 - W657F |
Special Link Register | ------ | SW000 - SW7FF |
File Register (Normal) | ------ | R00000 - R32767 |
File Register (Block switching is not necessary) | ------ | ZR0000000 - ZR1042431 |
File Register (0R-31R) | ------ | 0R00000 - 0R32767 |
------ | 1R00000 - 1R32767 |
------ | 2R00000 - 2R32767 |
: | : | :
------ | 30R00000 - 30R32767 |
------ | 31R00000 - 31R26623 |

*1The setting of the Multi CPU System is possible also in the system data area.

NOTE

- The notation of addresses differs depending on a selected Unit No.
  <Ex.>When 0 is selected for Unit No.,

  <Ex.>When 1 is selected for Unit No.,

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms