### Settings of External Device

Use the ladder software (MP720 Ver.7) to set up communication settings.

For details on communication settings, please refer to the manual of the External Device.

1. Start the ladder software.

2. Make a project file.
   In the [TypeSelect] area, set the [Series] and [Controller].

   Setup Items | Setup Description
   --- | ---
   Series | MP3000
   Controller | SIGMA-7C

3. Click [Module Configuration] to start [MC-Configurator].

4. Double-click [218IFD] on the CPU you want to use.

5. Click the [Transmission Parameters] tab.

6. In the [Transmission Parameters], set the [IP Address] and [Subnet Mask].

   Setup Items | Setup Description
   --- | ---
   IP Address | 192.168.0.1
   Subnet Mask | 255.255.255.0

7. For the CPU you want to use in [MC-Configurator], set [SVD] to [Circuit No1].

8. Write the settings to the External Device.

9. Turn ON the External Device again.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.