Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 1E | User-created cable | Total cable length: 500m or less
4E | BMJ-8P (Distributor) + User-created cable
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*c-2 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 1F | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + User-created cable | Total cable length: 500m or less
4F | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + BMJ-8P (Distributor) + User-created cable
1A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + User-created cable
4A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + BMJ-8P (Distributor) + User-created cable
1B | User-created cable
4B | BMJ-8P (Distributor) + User-created cable
PS5000 PS6000 (Optional Interface) PSA6000 *2 | 1G | User-created cable | Total cable length: 500m or less
4G | BMJ-8P (Distributor) + User-created cable

*c-2Except ST-6200 *2Only the COM port which can communicate by RS-422/485 (4 wire) can be used. IPC COM Port Recommended cables and connectors
Item | Type | Manufacturer
--- | --- | ---
Cable | FR-CB20**1 | Mitsubishi Electric Corporation
10BASE-T cable | SGLPEV-T0.5mmx4P*2 | Mitsubishi Electric Corporation
RJ45 connector | 5-554720-3 | Tyco Electronics AMP K.K.
RS-485 distributor | BMJ-8 | HACHIKO ELECTRIC CO.,LTD
BMJ-8P

*1Different figure (1, 3.or 5) is set in the * depending on the cable length. *2Do not use pin number 2 or 8.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.