### KV-700 Series

Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | 00000 - 59915 | 000 - 599 |  |
Output Relay |
Internal Auxiliary Relay |
Control Relay | CR0000 - CR3915 | CR00 - CR39 |
Timer (Contact) | T000 - T511 | ----- | - |
Counter (Contact) | C000 - C511 | ----- |
High-speed Counter Comparator (Contact) | CTC0 - CTC3 | ----- | *1
Timer (Setting Value) | ----- | TS000 - TS511 |  | *2
Counter (Setting Value) | ----- | CS000 - CS511 | *2
Timer (Current Value) | ----- | TC000 - TC511 | *2
Counter (Current Value) | ----- | CC000 - CC511 | *2
Data Memory | ----- | DM00000 - DM39999 | *3
Temporary Data Memory | ----- | TM000 - TM511 |
Control Memory | ----- | CM0000 - CM3999 |
Digital Trimmer | ----- | TRM0 - TRM7 | *1 *2
High-speed Counter (Current Value) | ----- | CTH0 - CTH1 | *2
High-speed Counter Comparator (Setting Value) | ----- | CTC0 - CTC3 | *2

*1Write disable

*232-bit device

*3To use DM20000 to DM39999, you need to install extended memory.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms