### Settings of External Device

Use the ladder software "Concept" for communication settings.

After selecting the External Device in Momentum Series in "PLC Selection" of "Concept", select "Modbus Port Settings" and perform the settings in the "Modbus Port Settings" dialog box.

Setup Items | Setup Description
--- | ---
Baud | 19200
Data Bits | 8
Stop Bits | 1
Parity | Even
Delay (ms) | 10
Address | 1
Head slot | 0
Mode | RTU
Protocol | RS232

NOTE

- Please refer to the manual of the ladder software for more detail on other setting description.

- Use an integer from 1 to 247 to enter the unit ID of the External Device.