### Settings of External Device

Use the LS ELECTRIC programming tool (XG5000) to define External Device communication settings.

Refer to your External Device manual for details.

1. Start up the configuration tool.

2. From the [Project] menu, select [New Project].

3. Configure the [PLC Series] and [CPU type], and click [OK].

4. From the tree view, double-click [Local Ethernet Parameter] and configure the Local Ethernet Parameter as follows.

Setup Items | Setup Description
--- | ---
IP Address | 192.168.0.1
Subnet mask | 255.255.255.0
Driver | XGT server

5. From the [Online] menu, select [Write] .

6. Select the External Device, and click [OK].

7. Restart the External Device.

NOTE

- Check with a network administrator about IP address.
  Do not set the duplicate IP address.