### FX3S

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Input Relay | X000 - X017 | X000 - X000 |  | *1 *2
Output Relay | Y000 - Y015 | - | *1
Auxiliary Relay | M0000 - M1535 | M0000 - M1520 |
Special Auxiliary Relay | M8000 - M8511 | M8000 - M8496 | *3
State | S0000 - S0255 | S0000 - S0240 |
Timer (Contact) | TS000 - TS137 | - |
Counter (Contact) | CS000 - CS031 CS200 - CS255 | - |
Timer (Current Value) | - | TN000 - TN137 |
Counter (Current Value) 1 | - | CN000 - CN031 |
Counter (Current Value) 2 | - | CN200 - CN255 | *4
Data Register | - | D0000 - D2999 |
Special Data Register | - | D8000 - D8511 | *3

*1Figures divisible by 20 (octal number) can be assigned to the word address.
For example, X0, X20, X40 ... X360

*2Writing cannot be made to the address, where Input Terminals are allocated on External Device, from Display.

*3Write protected addresses or unusable addresses (system usage) exist. If these addresses are written, the External Device may not function properly.

*4Data length of CN200 to CN255 is 32 bit.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms