### External Device Settings

For External Device communication settings, use the ladder software (CutyWaveII).

Refer to your External Device manual for details.

1. Start up the ladder software.

2. Open [Setting Parameters] window.

3. Select parameter to set.

4. Input setting value as shown below in each parameter.

   Parameter No. | Setting Value | Setup Description
   --- | --- | ---
   27 | 0 | Axis No.

5. Click [Export Data].

Communication settings are complete.