### K1G Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Data | 04096,00 - 36863,15 61440,00 - 65535,15 | 04096 - 36863 61440 - 65535 |  | *1 *2

*1When bits are written, the Display reads the corresponding word address from the External Device, sets particular bits of that word address to ON, and then returns the resulting address to the External Device. Note that the data may not be written correctly if you write to the word address using the External Device while the Display is reading data from, and writing data to, the External Device.

*2The Display uses the generic Modbus address format. Please refer to the following table for supported K1G series address types and address ranges.

K1G Series | Display
--- | ---
Address Types | Address Ranges | Address Ranges
Monitoring area | 0x1000 - 0x1FFF | 04096 - 08191
Setting area | 0x2000 - 0x2FFF | 08192 - 12287
Channel1 area | 0x3000 - 0x3FFF | 12288 - 16383
Channel2 area | 0x4000 - 0x4FFF | 16384 - 20479
Channel3 area | 0x5000 - 0x5FFF | 20480 - 24575
Channel4 area | 0x6000 - 0x6FFF | 24576 - 28671
Intensity area | 0x7000 - 0x7FFF | 28672 - 32767
Operation area | 0x8000 - 0x8FFF | 32768 - 36863
Special Function area | 0xF000 - 0xFFFF | 61440 - 65535

The External Device has 32 bit addresses. Read to or write from these 32 bit addresses in 32 bit units. For information about address length, please refer to the corresponding External Device manual.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms