Device | Bit address | Word address | 32 bits | Comments
--- | --- | --- | --- | ---
Class Instance Attribute Control Bit | Class: 0000h - FFFFh Instance: 00000 - 16383 Attribute: 00 - 63 Control address: 0000 - 4095 Bit: 0 - 31 | Class: 0000h - FFFFh Instance: 00000 - 16383 Attribute: 00 - 63 Control address: 0000 - 4095 | or *1 |

*1The high and low relationship of the stored data varies depending on the External Device. Refer to your External Device manual for details.

NOTE

- Please refer to the manual of the External Device for more details of the device. The device name notation differs in the manual of the BLUE and the External Device.

  BLUE | External Device
  Class | Command No.
  Instance | Instance
  Attribute | Attribute

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms

The address input area is shown below.

- For word addresses

*1 Not used if the command type is robot control (Class other than 0x04C0 to 0x04C3). (0000: reserved)

- For bit addresses

*1 Not used if the command type is robot control (Class other than 0x04C0 to 0x04C3). (0000: reserved)