Display (Connection Port) | Cable | Remarks
--- | --- | ---
GP-4116 (COM1) | 1G | User-created cable | Cable length: 1,000m or less. (Depends on master's capacity)
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 1A | Terminal Block Conversion Adapter by Pro-face CA3-ADPTRM-01 + User-created cable | Cable length: 1,000m or less. (Depends on master's capacity)
1I | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + User-created cable
1B | User-created cable
PS5000 PS6000 (Optional Interface) PSA6000 *8 | 1K | User-created cable | Cable length: 1,000m or less. (Depends on master's capacity)

*b-3Except ST-6200

*8Only the COM port which can communicate by RS-422/485 (2 wire) can be used.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.