### TCmini series (TC3-02)

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
External Input Relay | X000 - X00F | X00W - X00W |  | *1
External Output Relay | Y000 - Y00F | Y00W - Y00W | *1
Internal Relay | R000 - R37F | R00W - R37W | *1
Timer Relay | T000 - T13F | T00W - T13W | *1
Counter Relay | C000 - C13F | C00W - C13W | *1
Latch Relay | L000 - L03F | L00W - L03W | *1
Data Register | ------ | D000 - D24C | *1
T/C Register 1 | ------ | P000 - P13F | *1
T/C Register 2 | ------ | V000 - V15F | *1

*1Device format is as follows: Please refer to the manual of External Device for more detail.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms