### Settings of External Device

Use the TwinCAT for communication settings of the External Device. Please refer to the manual of the External Device for more details.

1. In the TwinCAT system, enter the following settings. Please refer to the manual of the External Device for more details.

   Setup Items | Setting Value
   --- | ---
   Address | 192.168.0.1
   AMS Net Id | 192.168.0.1.1.1

2. Add the Display's IP address and AMS NetId to the TwinCAT system.
   Right click the TwinCAT icon in the Notification Area, and select [Properties].

3. In the [AMS Router] tab, click [Add].

4. Enter the following settings and click [OK].

   Setup Items | Setting Value
   --- | ---
   AMS Net Id | 192.168.0.2.1.1
   Address | 192.168.0.2
   Transport | TCP/IP
   Port | 851

5. Restart the TwinCAT system.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address in the same network.