### Control/Compact/Flex Logix Series Native

Device |  | Bit Address | Word Address | 32bits | Remarks
--- | --- | --- | --- | --- | ---
BOOL | Single Tag | <TAGNAME> | - | - | *1 *2 *3
1D Array | <TAGNAME>[0]- <TAGNAME>[x-1]
INT | Single Tag | <TAGNAME>.00- <TAGNAME>.15 | <TAGNAME> |  | *1 *2
1D Array | <TAGNAME>[0].00- <TAGNAME>[x-1].15 | <TAGNAME>[0]- <TAGNAME>[x-1]
2D Array | <TAGNAME>[0,0].00- <TAGNAME>[x-1,y-1].15 | <TAGNAME>[0,0]- <TAGNAME>[x-1,y-1]
3D Array | <TAGNAME>[0,0,0].00- <TAGNAME>[x-1,y-1,z-1].15 | <TAGNAME>[0,0,0]- <TAGNAME>[x-1,y-1,z-1]
LINT | Single Tag | <TAGNAME>.00 - <TAGNAME>.63 | <TAGNAME> | *1 *2
1D Array | <TAGNAME>[0].00 - <TAGNAME>[x-1].63 | <TAGNAME>[0] - <TAGNAME>[x-1]
2D Array | <TAGNAME>[0,0].00 - <TAGNAME>[x-1,y-1].63 | <TAGNAME>[0,0] - <TAGNAME>[x-1,y-1]
3D Array | TAGNAME>[0,0,0].00 - <TAGNAME>[x-1,y-1,z-1].63 | <TAGNAME>[0,0,0] - <TAGNAME>[x-1,y-1,z-1]
REAL | Single Tag | - | <TAGNAME> | - | *1 *2
1D Array | <TAGNAME>[0]- <TAGNAME>[x-1]
2D Array | <TAGNAME>[0,0] <TAGNAME>[x-1,y-1]
3D Array | <TAGNAME>[0,0,0]- <TAGNAME>[x-1,y-1,z-1]
LREAL | Single Tag | - | <TAGNAME> | *1 *2
1D Array | <TAGNAME>[0]- <TAGNAME>[x-1]
2D Array | <TAGNAME>[0,0]- <TAGNAME>[x-1,y-1]
3D Array | <TAGNAME>[0,0,0]- <TAGNAME>[x-1,y-1,z-1]
DINT | Single Tag | <TAGNAME>.00- <TAGNAME>.31 | <TAGNAME> | *1 *2
1D Array | <TAGNAME>[0].00- <TAGNAME>[x-1].31 | <TAGNAME>[0]- <TAGNAME>[x-1]
2D Array | <TAGNAME>[0,0].00- <TAGNAME>[x-1,y-1].31 | <TAGNAME>[0,0] <TAGNAME>[x-1,y-1]
3D Array | <TAGNAME>[0,0,0].00- <TAGNAME>[x-1,y-1,z-1].31 | <TAGNAME>[0,0,0]- <TAGNAME>[x-1,y-1,z-1]
SINT | Single Tag | <TAGNAME>.0- <TAGNAME>.7 | <TAGNAME> |  | *1 *2
1D Array | <TAGNAME>[0].0- <TAGNAME>[x-1].7 | <TAGNAME>[0]- <TAGNAME>[x-1]
2D Array | <TAGNAME>[0,0].0- <TAGNAME>[x-1,y-1].7 | <TAGNAME>[0,0]- <TAGNAME>[x-1,y-1]
3D Array | <TAGNAME>[0,0,0].0- <TAGNAME>[x-1,y-1,z-1].7 | <TAGNAME>[0,0,0]- <TAGNAME>[x-1,y-1,z-1]
STRING | Single Tag | - | <TAGNAME> | - | *1 *2
1D Array | <TAGNAME>[0]- <TAGNAME>[x-1]
2D Array | <TAGNAME>[0,0]- <TAGNAME>[x-1,y-1]
3D Array | <TAGNAME>[0,0,0]- <TAGNAME>[x-1,y-1,z-1]

*1<TAGNAME>: Tag Name including structure name in case of structure. The maximum number of characters for Tag Name is 255 including delimiters and element number.

Ex.) BOOL type single tag: "BOOLTAG"

BOOL array element: "BOOLARRAY[0012]"

INT type single tag: "INTTAG"

DINT type single address: "DINTTAG.30"

REAL type 3Darray: "REALARRAY[1,2,3]"

DINT from TIMER structure: "TIMERTAG.PRE"

SINT from STRING structure: "STRINGTAG.DATA[00]"

BOOL from User Defined Structure: "USERSTRUCTURE_A.USERSTRUCTURE_B.MYTIMER.EN"

*2Array Element Number: Number of array element is included in the controller tag information. Since the element number starts from 0, maximum element number is [Element Number - 1].

Ex.) INTARRAY INT[256,256] can be used in the range of INTARRAY[0-255,0-255].

*3BOOL type array: Available to define only 1 dimension. Number of array element can be specified by multiples of 32.

To use controller tags set up in the Studio 5000 (former RSLogix5000) software on BLUE, the L5K file needs to be imported. The L5K file is exported by the Studio 5000 software. The L5K data imported into BLUE is saved as a variable.

IMPORTANT

- BLUE will import L5K files for Studio 5000 software version 13 to 21 and 28 to 37.
- When controller tags created with the Studio 5000 software have settings to limit external access, please allow for external access.

In addition to controller scope or global tags, Studio 5000 also provides for Program Scope Tags which are only valid within the PLC program they are created. BLUE will import these Program Scope Tags from L5K files exported from Studio 5000.

The following derivative data types are provided by Studio 5000, and are supported in BLUE.

- Predefined data type: a structure data type defined in Studio 5000. Predefined data types for Studio 5000. (FS, LS, OV, and ER of TIMER Predefined types are not supported).

- Module defined data type: Data type defined according to a physical module being used in an Studio 5000 project. BLUE determines the tags and data types needed for module definitions found in the L5K file. (Please refer to "Data Type Defined Module List" for all modules supported in BLUE).

- User defined data type: data type defined by the user in Studio 5000. Its definition is exported into the L5K file.

- Alias: A tag name which refers to another tag or alias on the External Device.

- Add-on-Instruction Data Type

Add-on-Instruction Data Type members specified with a Usage value of "InOut" will not be imported into BLUE.

- Custom String Data Type

The Ethernet/IP driver's Custom String Data Type supports text up to 400 characters. (The STRING device supports text up to 82 characters.)

#### Data Type Defined Module List

##### Modules that do not generate tags or data type/structures on import

Embedded | 1756-L1 | 1756-L53
1756-HYD02 | 1756-EWEB/A | 1768-ENBT/A
1756-L55 | 1756-L60M03SE | 1756-L61
1756-L61S | 1756-L62 | 1756-L62S
1756-LSP | 1756-L63 | 1756-L64
1756-M02AE | 1756-M02AS | 1756-M03SE
1756-M08SE | 1756-MO8SEG | 1756-M16SE
1768-L43 | 1768-EWEB/A | 1769-L20
1769-L30 | 1769-L31 | 1769-L32E Ethernet Port
1769-L32E | 1769-L35CR | 1769-L35E
1769-L35E Ethernet Port | 1788-ENBT/A | 1788-EWEB/A
1789-L60 | 1794-L33 | 1794-L34
CompactBus | Emulator | ETHERNET-BRIDGE
1769-L23E-QB1 Ethernet Port | 1769-L23E-QBFC1 Ethernet Port | Drivelogix5730 Ethernet Port
1769-L30ER | 1769-L30ERM | 1769-L30ER-NSE
1769-L33ER | 1769-L36ERM | 1756-63S
1756-L72S | 1756-L73S | 1768-CNB/A
1756-L71 | 1756-L71S | 1756-L72
1756-L73 | 1756-L74 | 1756-L75
1769-L30ERMS | 1769-L33ERM | 1769-L33ERMS
1769-L36ERMS | 1769-L37ERM | 1769-L37ERMO
1769-L37ERMOS | 1769-L37ERMS | 1769-L38ERM
1769-L38ERMS | --- | ---

##### Modules that generate controller tags or data type/structures on import

NOTE

- Depending on your system structure, controller tags may not generate properly.

1734-ACNR/A | 1734-IA2/C | 1734-IB2/C
1734-IB4/C | 1734-IB8/C | 1734-IE2C/C
1734-IE2V/C | 1734-IJ/C | 1734-IK/C
1734-IM2/C | 1734-IR2/C | 1734-IT2I/C
1734-IV2/C | 1734-IV4/C | 1734-IV8/C
1734-MODULE | 1734-OA2/C | 1734-OB2/C
1734-OB2E/C | 1734-OB2EP/C | 1734-OB4/C
1734-OB4E/C | 1734-OB8/C | 1734-OB8E/C
1734-OE2C/C | 1734-OE2V/C | 1734-OV2E/C
1734-OV4E/C | 1734-OV8E/C | 1734-OW2/C
1734-OW4/C | 1734-OX2/C | 1734-SSI/C
1734-VHSC24/C | 1734-VHSC5/C | 1738-ACNR/A
1738-IA2M12AC3/A | 1738-IA2M12AC4/A | 1738-IB2M12/A
1738-IB4M12/A | 1738-IB4M8/A | 1738-IB8M12/A
1738-IB8M23/A | 1738-IB8M8/A | 1738-IE2CM12/A
1738-IE2VM12/A | 1738-IJM23/A | 1738-IR2M12/A
1738-IT2IM12/A | 1738-IV4M12/A | 1738-IV8M12/A
1738-IV8M23/A | 1738-IV8M8/A | 1738-MODULE
1738-OA2M12AC3/A | 1738-OB2EM12/A | 1738-OB2EPM12/A
1738-OB4EM12/A | 1738-OB4EM8/A | 1738-OB8EM12/A
1738-OB8EM23/A | 1738-OB8EM8/A | 1738-OE2CM12/A
1738-OE2VM12/A | 1738-OV4EM12/A | 1738-OW4M12/A
1738-OW4M12AC/A | 1738-SSIM23/A | 1738-VHSC24M23/A
1747-ASB | 1756-CFM/A | 1756-CN2/A
1756-CN2/B | 1756-CN2R/A | 1756-CN2R/B
1756-CNB/A | 1756-CNB/B | 1756-CNB/D
1756-CNB/E | 1756-CNBR/A | 1756-CNBR/B
1756-CNBR/D | 1756-CNBR/E | 1756-DHRIO/B
1756-DHRIO/C | 1756-DHRIO/D | 1756-DMA30
1756-DMA31 | 1756-DMA50 | 1756-DMB30
1756-DMD30 | 1756-DMF30 | 1756-DNB
1756-EN2F/A | 1756-EN2T/A | 1756-ENBF/A
1756-ENBT/A | 1756-ENET/B | 1756-HSC
1756-IA16 | 1756-IA16I | 1756-IA8D
1756-IB16 | 1756-IB16D | 1756-IB16I
1756-IB16ISOE | 1756-IB32 | 1756-IB32/A
1756-IB32/B | 1756-IC16 | 1756-IF16
1756-IF4FXOF2F/A | 1756-IF4FXOF2F/B | 1756-IF6CIS/A
1756-IF6I | 1756-IF8 | 1756-IG16/A
1756-IH16I | 1756-IH16ISOE | 1756-IM16I
1756-IN16 | 1756-IR6I | 1756-IT6I
1756-IT6I2 | 1756-IV16/A | 1756-IV32/A
1756-MODULE | 1756-OA16 | 1756-OA16I
1756-OA8 | 1756-OA8D | 1756-OA8E
1756-OB16D | 1756-OB16E | 1756-OB16I
1756-OB16IS | 1756-OB32 | 1756-OB8
1756-OB8EI | 1756-OC8 | 1756-OF4
1756-OF6CI | 1756-OF6VI | 1756-OF8
1756-OG16/A | 1756-OH8I | 1756-ON8
1756-OV16E/A | 1756-OV32E/A | 1756-OW16I
1756-OX8I | 1756-PLS/B | 1756-REG
1756-SYNCH/A | 1769-HSC | 1769-HSC/A
1769-IA16 | 1769-IA16/A | 1769-IA8I
1769-IA8I/A | 1769-IF4/A | 1769-IF4/B
1769-IF4I/A | 1769-IF4XOF2/A | 1769-IF8/A
1769-IM12/A | 1769-IQ16/A | 1769-IQ16F/A
1769-IQ32/A | 1769-IQ6XOW4/A | 1769-IQ6XOW4/B
1769-IR6/A | 1769-IT6/A | 1769-MODULE
1769-OA16/A | 1769-OA8/A | 1769-OA8/B
1769-OB16/A | 1769-OB16/B | 1769-OB16P/A
1769-OB16P/B | 1769-OB32/A | 1769-OB8/A
1769-OF2/A | 1769-OF2/B | 1769-OF4CI/A
1769-OF4VI/A | 1769-OF8C/A | 1769-OF8V/A
1769-OV16/A | 1769-OV16/B | 1769-OW16/A
1769-OW8/A | 1769-OW8/B | 1769-OW8I/A
1769-OW8I/B | 1769-SDN/A | 1769-SDN/B
1771-ASB | 1788-EN2DN/A | 1794-ACN15/C
1794-ACNR15/C | 1794-AENT/A | 1794-AENT/B
1794-ASB | 1794-IA16/A | 1794-IA8/A
1794-IA8I/A | 1794-IB10XOB6/A | 1794-IB16/A
1794-IB16XOB16P/A | 1794-IB32/A | 1794-IB8/A
1794-IB8S/A | 1794-IC16/A | 1794-ID2/B
1794-IE4XOE2/B | 1794-IE8/B | 1794-IF2XOF2I/A
1794-IF4I/A | 1794-IJ2/A | 1794-IM8/A
1794-IP4/B | 1794-IR8/A | 1794-IRT8
1794-IRT8/A | 1794-IT8/A | 1794-IV16/A
1794-OA16/A | 1794-OA8/A | 1794-OA8I/A
1794-OB16/A | 1794-OB16P/A | 1794-OB32P/A
1794-OB8/A | 1794-OB8EP/A | 1794-OC16/A
1794-OE4/B | 1794-OF4I/A | 1794-OM8/A
1794-OV16/A | 1794-OV16P/A | 1794-OW8/A
1794-VHSC/A | 1797-ACNR15/C | 1797-IBN16/A
1797-IE8/A | 1797-IE8NF/A | 1797-IJ2/A
1797-IRT8/A | 1797-OB4D/A | 1797-OE8/A
56AMXN | CIP-MODULE | ETHERNET-MODULE
FlexBus | FLEX-MODULE | RIO-ADAPTER
1756-OB8I | EtherNet/IP | 1734-AENT/A
1738-AENT/A | 1794-OE12/A | 1794-IT8/B
1769-IQ32T/A | 1769-L16ER-BB1B | 1769-L18ER-BB1B
1769-L18ERM-BB1B | 1769-L23E-QB1 | 1769-L23E-QBFC1
1769-L23-QBFC1 | 1769-L24ER-QB1B | 1769-L24ER-QBFC1B
1769-L27ERM-QBFC1B | 5069-IB16/A | 5069-OB16/A
5069-L340ER | 1756-ENET/A | 1756-EN2TR
1734-AENTR/B | --- | ---

NOTE

- For tag import procedures, see the following.
  Importing Symbols from External Devices

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms