### Setting of External Device

Use the Shenzhen Inovance ladder software (AutoShop Ver.3.01 or later) to configure communication settings for the External Device.

Refer to your External Device manual for details.

1. Start up the ladder software.

2. Select [New Project].

3. Configure the setup items as follows, and click [OK].

   Setup Items | Setup Description
   --- | ---
   Project Name | Enter the project name.
   Project Path | Select the save destination.
   PLC Type | Select the series of the External Device.

4. In tree view, from [Communication Config] click the COM port that you will use and display the [COM Config] dialog box.

5. Configure the setup items as follows.

   Setup Items | Setup Description
   --- | ---
   Protocol | MODBUS-RTU Slave Site
   Baud rate | 9600
   Data Length | 8bit
   Parity | None
   Stop Bit (s) | 2bit
   Station | 1
   Time Out | 10

NOTE

- When using COM1, COM2 or COM3, select [Operate communication setting].

6. Click [OK] to complete the configuration.

7. Click [Write] to write the settings to the External Device.