### External Device Settings

Use the configuration tool (KV BUILDER/Ver. 4.70) for External Device communication settings. Refer to your External Device manual for details.

1. Start up the configuration tool.

2. From the [File] menu, select [New Project], enter a project name, and then click [OK].

3. In the [Change Device] dialog box, if extended memory is installed, select "KV-700+M"; if not, select "KV-700". Then click [OK].

4. In the dialog box that appears, click [Yes] to move to the Unit Editor.

5. Click the [Unit selection (2)] tab, select "KV-LE20A", and then drag and drop the unit between the CPU and the end unit.

6. With KV-LE20A selected, switch to the [Unit setup (3)] tab, and set as follows.

   Setup Items | Settings
   First DM No. | DM10000
   Speed | 100/10 Mbps (automatic)
   IP Address | 192.168.0.1
   Subnet Mask | 255.255.255.0
   Port No. (HOST Link) | 8501

7. From the [File] menu, select [Save and Exit] to return to the editor mode.

8. From the [Monitor/Simulator] menu, select [Convert ➝ Move ➝ Monitor].

9. Check [Unit setting information], and then click [Exec]. The setting information is transferred.

This completes the setting of the External Device.

NOTE

- Check with your network administrator about the IP address you want to use.
- Do not duplicate IP addresses on the same network.