NOTE

- When using a NX Series, from the [Series] list select [NJ/NX].

### External Device Settings

Use the ladder software (Sysmac Studio) to configure communication settings for the External Device.

Refer to your External Device manual for details.

1. Start up the ladder software.

2. Click the [Configuration] of the [Multiviewer Explorer].

3. Double click [Controller Setup].

4. Double click [Built-in EtherNet/IP Port Setings] to display the setup screen.

5. Select [Use the Port2] from [IP Address - Port2].

6. Select [Fixed settings] to set the IP address as follows.

Setup Items | Setup Description
--- | ---
IP address | 192.168.0.1
Subnet mask | 255.255.255.0

7. Transfer the communication settings to the External Device.

NOTE

- Check with a network administrator about IP address and subnet mask you want to use. Do not set the duplicate IP address.