### FP0H Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
External Input (X) | X0000 - X109F | WX000 - WX109 |  | *1
External Output (Y) | X0000 - X109F | WY000 - WY109 |
Internal Relay (R) | R0000 - R511F | WR000 - WR511 |
Link Relay (L) | L0000 - L127F | WL000 - WL127 |
Special Internal Relay (R) | R9000 - R951F | WR900 - WR951 | *1
Timer (T) | T0000 - T1023 | -------- | *1
Counter (C) | C0000 - C1023 | ------- | *1
Timer/Counter (Setting Value) | ----- | SV0000 - SV1023 |
Timer/Counter (Elapsed Value) | ----- | EV0000 - EV1023 |
Data Register (DT) |  | DT00000 - DT65532 |
Special Data Register (DT) |  | DT90000 - LD90999 |
Link Data Register (LD) |  | LD000 - LD255 |

*1Write disable

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms