Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) STM6000 (COM1) PC/AT IPC*2 | 7A | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB | Cable length from SIO converter to External Device: 100m or less
7B | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
7C | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 1 + Junction by AMP 5-1473574-4 + User-created cable 2 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
7D | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 1 + Junction by AMP 5-1473574-4 + User-created cable 2 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB | Cable length from SIO converter to External Device: 100m or less
7E | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Insulated PIO terminal block by IAI Corporation RC*-TU-PIO-* + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO***-H6 or CB-ERC-PWBIO***-RB-H6
GP-4115 (COM1) | 7F | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB | Cable length from SIO converter to External Device: 100m or less
7G | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
7H | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 1 + Junction by AMP 5-1473574-4 + User-created cable 2 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
7I | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 1 + Junction by AMP 5-1473574-4 + User-created cable 2 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
7J | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable by IAI Corporation CB-RCA-SIO050 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable + Insulated PIO terminal block by IAI Corporation RC*-TU-PIO-* + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO***-H6 or CB-ERC-PWBIO***-RB-H6

*2Only the COM port which can communicate by RS-232C can be used.

IPC COM Port

NOTE

- RS232C conversion unit (RCB-CV-MW) and communication cable (CB-RCA-SIO050) are accessories of PC Interface Software (RCM-101-MW) by IAI Corporation.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.