Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 2G | User-created cable 1 + Junction by AMP 5-1473574-4 + Controller link cable by IAI Corporation CB-RCB-CTL002 | Cable length: 100m or less
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 2I | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1*8 + User-created cable 1 + Junction by AMP 5-1473574-4 + Controller link cable by IAI Corporation CB-RCB-CTL002 | Cable length: 100m or less
2B | User-created cable 1 + Junction by AMP 5-1473574-4 + Controller link cable by IAI Corporation CB-RCB-CTL002
PS5000 PS6000 (Optional Interface) PSA6000 *9 | 2K | User-created cable 1 + Junction by AMP 5-1473574-4 + Controller link cable by IAI Corporation CB-RCB-CTL002 | Cable length: 100m or less

*b-3Except ST-6200

*8When using a Terminal Block Conversion Adapter (CA3-ADPTRM-01) instead of the RS-422 Terminal Block Conversion Adapter, refer to Cable Diagram 2A.

*9Only the COM port which can communicate by RS-422/485 (2 wire) can be used.

IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.