### EHV Series

Device | Bit Address | Word Address | Double Word Address | 32 bits | Remarks
--- | --- | --- | --- | --- | ---
External Input | X00000-X05A95 | WX0000-WX05A7 | DX0000-DX05A6 |  | *1 *2
External Output | Y00000-Y05A95 | WY0000-WY05A7 | DY0000-DY05A6 | *2
Remote Input Relay | X10000-X45A95 | WX1000-WX45A7 | DX1000-DX45A6 | *1 *3
Remote Output Relay | Y10000-Y45A95 | WY1000-WY45A7 | DY1000-DY45A6 | *3
Extension External Input | EX00000-EX5A7FF | WEX0000-WEX5A7F | DEX0000-DEX5A7E | *1
Extension External Output | EY00000-EY5A7FF | WEY0000-WEY5A7F | DEY0000-DEY5A7E |
Internal Output | R000-R7BF | - | - |
Special Internal Output | R7C0-RFFF | - | - |
Data Area | M00000-M7FFFF | WM0000-WM7FFF | DM0000-DM7FFE |
First CPU Link | L00000-L03FFF | WL0000-WL03FF | DL0000-DL03FE |
Second CPU Link | L10000-L13FFF | WL1000-WL13FF | DL1000-DL13FE |
Third CPU Link | L20000-L23FFF | WL2000-WL23FF | DL2000-DL23FE |
Fourth CPU Link | L30000-L33FFF | WL3000-WL33FF | DL3000-DL33FE |
Fifth CPU Link | L40000-L43FFF | WL4000-WL43FF | DL4000-DL43FE |
Sixth CPU Link | L50000-L53FFF | WL5000-WL53FF | DL5000-DL53FE |
Seventh CPU Link | L60000-L63FFF | WL6000-WL63FF | DL6000-DL63FE |
Eighth CPU Link | L70000-L73FFF | WL7000-WL73FF | DL7000-DL73FE |
On Delay Timer | TD0000-TD2559 | - | - |
Off Delay Timer | TDN0000-TDN2559 | - | - |
Single-shot Timer | SS0000-SS2559 | - | - |
Watchdog Timer | WDT0000-WDT2559 | - | - |
Mono Stable Timer | MS0000-MS2559 | - | - |
Retentive Timer | TMR0000-TMR2559 | - | - |
Up-down Counter | CT000-CT511 | - | - |
Up Counter | CU000-CU511 | - | - |
Link Counter | RCU000-RCU511 | - | - |  |
Timer Counter (Elapsed Value) | - | TC0000-TC2559 | - |
Word Internal Output | WR0000.0- WREFFF.F | WR0000-WREFFF | DR0000-DREFFE |
Special Word Internal Output | WRF000.0- WRFFFF.F | WRF000- WRFFFF | DRF000-DRFFFE |
Data Area | WN00000.0-WN1FFFF.F | WN00000-WN1FFFF | DN00000-DN1FFFE |

*1Write disable

*2Specify as shown below.

(Example) External input unit No.1, Slot No.2, Internal Module Bit No.34

(Example) External input unit No.1, Slot No.2, Internal Module Word No.3

*3Specify as shown below.

(Example) Remote External Input Remote Master No.1, Remote Slave No.2, Slot No.3, Internal Module Bit No.45

(Example) Remote External Input Remote Master No.1, Remote Slave No.2, Slot No.3, Internal Module Word No.4

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms