Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
External Input | X000 - XFFF | XW000 - XWFF0 |  | *1
External Output | Y000 - YFFF | YW000 - YWFF0 | *1
Internal Register | R000 - RFFF | RW000 - RWFF0 | *1
Global Link Register | G000 - GFFF | GW000 - GWFF0 | *1
Event Register | E000 - EFFF | EW000 - EWFF0 | *1
Keep Relay | K000 - KFFF | KW000 - KWFF0 | *1
System Register | S000 - SBFF | SW000 - SWBF0 | *1
On-delay Register | T000 - T1FF | TW000 - TW1F0 | *1
One-shot Timer | U000 - U0FF | UW000 - UW0F0 | *1
Up/Down Counter | C000 - C0FF | CW000 - CW0F0 | *1
Transfer Register | J000 - JFFF | JW000 - JWFF0 | *1
Receive Register | Q000 - QFFF | QW000 - QWFF0 | *1
Extended Internal Register | M000 - MFFF | MW000 - MWFF0 | *1
Extended Internal Register | A000 - AFFF | AW000 - AWFF0 | *1
Timer Calculation Value | ----- | TC000 - TC1FF |
Timer Setting Value | ----- | TS000 - TS1FF |
One-shot Timer Calculation Value | ----- | UC000 - UC0FF |
One-shot Timer Setting Value | ----- | US000 - US0FF |
Counter Calculation Value | ----- | CC000 - CC0FF |
Counter Setting Value | ----- | CS000 - CS0FF |
Work Register | ----- | FW000 - FWBFF |
Data Register | ----- | DW000 - DWFFF |
Work Register | LB0000 - LBFFFF | LBW0000 - LBWFFF0 |
Ladder Converter Special Work Register | LR0000 - LR0FFF | LRW0000 - LRW0FF0 |
Ladder Converter Special Work Register (Edge) | LV0000 - LV0FFF | LVW0000 - LVW0FF0 |
Word Special Work Register | ----- | LWW0000 - LWWFFFF |
Long Word Special Work Register | ----- | LLL0000 - LLL1FFF | *2
Single Precision Floating Decimal Point Work Register | ----- | LF0000 - LF1FFF | *2 *3
Word Special Work Register (Power-cut Retain) | ----- | LXW0000 - LXW3FFF |
Long Word Special Work Register (Power-cut Retain) | ----- | LML0000 - LML1FFF | *2
Single Precision Floating Decimal Point Work Register (Power-cut Retain) | ----- | LG0000 - LG1FFF | *2 *3
Direct Memory Address*4 | ----- | DM00000000 - DMFFFFFFFE |

*1Based on the specifications of the External Device, 0th bit is assigned as the most significant bit (MSB), and 15th bit as the least significant bit (LSB). Therefore, if you set the 0th bit to ON, 32768 (0x8000) is written into the word device with the bit at the beginning. If you set X000 to ON when assigning bits to the Display, the bit device X000 on the External Device will be set to ON. The word device XW000 of the Display and External Device is set to "32768 (0x8000)". *232-bit device. *3Single-precision floating point device. *4Used to access the memory address of the External Device.

IMPORTANT:

- When you access the External Device using the Direct Memory Address, do not access the memory address that the system uses. If you conduct it, an error may occur. For details concerning the address, refer to the manual attached to the External Device.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms