### 3H

1:1

1:n

Legend | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: D-sub 9 pin (plug) External Device side: Terminal Block | Connect the shield to FG (Shell).

IMPORTANT:

- Use the lead wire to connect between "-" terminal and "E" terminal in the External Device which terminates the connection.
- The 5V output (Pin #6) on the Display is the power for the Siemens AG's PROFIBUS connector. Do not use it for other devices.

NOTE

- Cable length: 1200m or less.