### 4A

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) External Device side: D-Sub 25 pin (socket) | Instead of connecting the Display (FG), connect the Shield to the Shell.
(2) | RS 232 D tap link cable by Schneider Electric TSX SCP CC 1030 (3m) |
(3) | PCMCIA card for RS232C by Schneider Electric TSX SCP 111 |

NOTE

- The cable length have to be 15m or less.
  Total length for TSX SCP CC 1030 and User-created cable.