### Settings of External Device

Use the LS ELECTRIC setting tool (XG-PD Editor) to configure communication settings for the External Device.

Refer to your External Device manual for details.

##### EtherNet module Setting

1. Start up the setting tool.

2. From the [File] menu, select [New File], and create the project.

3. From the [Online] menu, select [Connect].

4. From the [Online] menu, select [Read IO Information].

5. Double-click [FEnet] displayed in the tree view and set EtherNet module.

Setup Items | Setup Description
--- | ---
IP Address | 192.168.0.1
Subnet mask | 255.255.255.0
Driver | XGT server

6. Select [Write Parameter(Standard Settings,HS Link,P2P)] from the [Online] menu after selecting [Connect] from the [Online] menu and connecting External Device with communication setting software.

7. Select [Reset] from the [Online] menu, and reboot External Device.

NOTE

- Check with a network administrator about IP address.
  Do not set the duplicate IP address.