### FP Series (Except FP7 Series)

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Input Relay | X0000 - X511F | WX000 - WX511 |  | *1
Output Relay | Y0000 - Y511F | WY000 - WY511 |
Internal Relay | R0000 - R886F | WR000 - WR886 |
Link Relay | L0000 - L639F | WL000 - WL639 |
Special Relay | R9000 - R910F | WR900 - WR910 | *1
Timer (Contact) | T0000 - T3071 | -------- | *1
Counter (Contact) | C0000 - C3071 | ------- | *1
Timer/Counter (Setting Value) | ----- | SV0000 - SV3071 |
Timer/Counter (Elapsed Value) | ----- | EV0000 - EV3071 |
Data Register |  | DT00000 - DT10239 | *3
Link Register |  | LD0000 - LD8447 |
File Register |  | FL00000 - FL32764 |
Special Data Register |  | DT90000 - DT90511 | *1*4

*1Write disable *3The following addresses of DT09000 are handled as special data register in FP0 (C10/C14/C16/C32/SL1), FP1, FP-e, FP-M, FP3. *4Can be used only in FP0 (T32C), FPS, FP2, FP2SH, FP10S, FP10SH.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms