### 1E

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal Block External Device side: Terminal Block |

NOTE

- For the shield ground, be sure to use the ground terminal on the External Device.
- Turn on the termination resistor switch on the External Device located at the end.
- Cable length: 50m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON