Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 4G | User-created cable |
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 4B | User-created cable |
PS5000 PS6000 (Optional Interface) PSA6000 *5 | 4K | User-created cable |

*b-3Except ST-6200 *5Only the COM port which can communicate by RS-422/485 (2 wire) can be used. IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.