### 9K

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) Junction side: e-CON connector (plug) | Instead connecting the Display (FG), connect the Shield to the Shell.
(2) | Junction by AMP 5-1473574-4 |
(3) | Network Connection Cable by IAI Corporation CB-ERC2-CTL001 Connector Junction side: e-CON connector (plug) |
(4) | Power & I/O Cable by IAI Corporation CB-ERC2-PWBIO*** or CB-ERC2-PWBIO***-RB |
(5) | Termination resistance Connector Junction side: e-CON connector (plug) |
(6) | User-created cable Connector Junction side: e-CON connector (plug) |

NOTE

- Cable length: 100m or less

*1 We recommend the IAI Corporation CB-ERC2-PWBIO*** or CB-ERC2-PWBIO***-RB as the Power & I/O Cable.