### 6H)

Legend | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: D-sub 9 pin (plug) External Device side: Terminal block | Connect the shield to FG (Shell).

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power supply for Siemens AG's PROFIBUS connector. Do not use it for other devices.

NOTE

- Termination resistance of 120Ω is built into the External Device.
- For the External Device connector, use the XA connector (XAP-03V-1) by J.S.T. Mfg.
- Cable length: 500m or less.