### 14G

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: RJ-45 connector |

NOTE

- Please turn on the DIP Switch 1 to enable build-in resistance (100Ω) on the remotest External Device side.

- Cable length: 500m or less

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON