### MEMOCON Micro

Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Coil (Output/Internal) | 00001-01531 | - |  | *1 *2
Input Relay | 10001-10511 | - | *1 *2 *3
Input Register | - | 30001-30047 | *3
Output/Holding Register | - | 40001-41871 |

*1When you write the bit address, the Display reads the word address corresponding to that of the External Device first. Then, it changes the target bit address among the word data once read and returns the word data to the External Device. Note that the correct data may not be read if you change the word address value in the ladder program while the Display reads the data of the External Device and returns it to the External Device.

*2Specification using the word address is also available.

*3Write disable

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms