### Setting of External Device

Communication setting of External Device using MODE selector switch, Address switch and setting tool (PC Interface Software for RC) of External Device.

Please refer to the manual of the External Device for more details.

##### Procedure

1. Set the MODE selector switch of External Device as follows.

   MODE selector switch | Setting Value
   --- | ---
   Selector switch | MANU

2. Set the Address switch of External Device as follows.

   Address switch | Setting Value
   --- | ---
   ADRS | 0

3. Start up the setting tool.

4. Select [Teach mode1 (Safety speed effective/PIO start prohibition)] of a window to select manual operation mode.

5. Expand the axis number to be set from the tree view and click [Parameter].

6. Set [SIO Baudrate[bps]] of External Device as follows.

   Setup Item | Setting Value
   --- | ---
   SIO Baudrate[bps] | 38400

7. Select [Send to Controller] from the [Parameter] menu and send the set contents to the controller.