### 1D)

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: RJ-45 |

NOTE

- The cable length is normally 1000m or less, depending on the External Device. Refer to your External Device manual for details.
- The connection method and termination resistance depends on the External Device.
- The termination resistance on the Display is not isolated.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON