Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
I/O Relay | 00000 - 00915 | 000 - 009 |  |
07000 - 17915 | 070 - 179 |
Internal Auxiliary Relay | 01000 - 01915 | 010 - 019 |
03000 - 06915 | 030 - 069 |
Special Auxiliary Relay | 02000 - 02915 | 020 - 029 |
Timer (Contact) | T000 - T249 | ------ |
Counter (Contact) | C000 - C249 | ------ |
High-speed Counter Comparator (Contact) | CTC0 - CTC3 | ------ | *1
Timer (Current Value) | ------ | TC000 - TC249 |
Timer (Setting Value) | ------ | TS000 - TS249 |
Counter (Current Value) | ------ | CC000 - CC249 |
Counter (Setting Value) | ------ | CS000 - CS249 |
Data Memory | ------ | DM0000 - DM1999 |
Temporary Data Memory | ------ | TM00 - TM31 |
Digital Trimmer | ------ | AT0 - AT1 | *1
High-speed Counter (Current Value) | ------ | CTH0 - CTH1 |
High-speed Counter Comparator (Setting Value) |  | CTC0 - CTC3 |

*1Write disable