### Setting of External Device

Use the GPP function software by Mitsubishi Electric Corporation to perform the communication settings as below.

1. Double-click [PC Parameter] from [Parameter] to select [Serial Communication Settings].

2. Set as below.

   Setup Items | Settings
   Use Serial Communication Function*1 | Use
   Baud Rate | 19.2Kbps
   Sum Check | Enable
   Transmission Wait Time | No Wait
   Write Setting during RUN | Enable

*1Check the checkbox to make other setting items become available to set.

NOTE

- Available when using the unit (Q02UCPU) whose first 5 digits of the serial No. is "10102" or later, and GX Developer version 8.76E or later.