### Setting Example

Use the Control Techniques configuration tool (CTSoft Ver.01.10.02) for External Device communication settings. Refer to your External Device manual for details.

1. Start up the configuration tool.

2. Create a new project.

3. From [Parameters] select [SM-Applications Plus] for the slot number to use in the tree view and display the dialog box.

4. Double-click a parameter you want to set and display the [Edit Parameter] dialog box.

5. Set each item as shown below and click [OK]

   Parameter | Setup Items | Setting
   --- | --- | ---
   05 | RS-485 address | 1
   06 | RS-485 mode | 15
   07 | RS-485 baud rate | 6: 19200
   08 | RS-485 turnaround delay | 2
   09 | RS-485 Tx enable delay | OFF

6. Download the communication settings to the External Device.

7. Reset the External Device.

8. Save the communication settings in the External Device.

9. Reboot the External Device.

NOTE

- Use an integer from 1 to 247 to enter the unit ID of the External Device.