Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) STM6000 (COM1) PC/AT IPC*2 | 7A | D-Shell adapter by Schneider Electric 110 XCA 203 00 + RS232 communication cable RJ45 to RJ45 by Schneider Electric 110 XCA 282 01(1m), 110 XCA 282 02(3m) or 110 XCA 282 03(6m) | Cable length: 9.5m or less.
7D | Schneider Electric XBT ZG919 + Schneider Electric XBT Z9711 |
GP-4115 (COM1) | 7B | User-created cable | Cable length: 9.5m or less.

*2Only the COM port which can communicate by RS-232C can be used.

IPC COM Port