### Setting of External Device

Use the configuration tool (S10V ET.NET SYSTEM) for communication settings of the External Device.

1. Set the [MODU No.] rotary switch on the link I/F unit to "2", and then activate the External Device.

2. Connect an RS-232C cable from your PC to the CPU unit of the External Device, and then start up the configuration tool.

3. Select "RS-232C" from [Setup by module], and then click [OK].

4. Click [Set IP Address] in the [Setup by module] dialog box displayed.

5. Set the communication settings in the [Set IP Address] dialog box displayed.

   Setup Items | Setup Description
   --- | ---
   Module | ET.NET (Main)
   IP Address | 192.168.0.1
   Subnetmask | 255.255.255.0

6. Click [Register].

NOTE

- The LQE720 requires the following CPU revisions:
  LQP510:Revision.H or later
  LQP520: Revision.F or later
- For LQP520, LQP510 is also required.