Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) STM6000 (COM1) PC/AT IPC*2 | 3A | User-created cable + SIO converter by IAI Corporation RC*-TU-SIO-* + Controller link cable by IAI Corporation CB-RCB-CTL002 | Cable length from Display to SIO converter: 15m or less Cable length from SIO converter to External Device: 100m or less
3B | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Junction by AMP 5-1473574-4 + Controller link cable by IAI Corporation CB-RCB-CTL002
3C | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Junction by AMP 5-1473574-4 + Controller link cable by IAI Corporation CB-RCB-CTL002
GP-4115 (COM1) | 3D | User-created cable + SIO converter by IAI Corporation RC*-TU-SIO-* + Controller link cable by IAI Corporation CB-RCB-CTL002 | Cable length from Display to SIO converter: 15m or less Cable length from SIO converter to External Device: 100m or less
3E | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Junction by AMP 5-1473574-4 + Controller link cable by IAI Corporation CB-RCB-CTL002
3F | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Junction by AMP 5-1473574-4 + Controller link cable by IAI Corporation CB-RCB-CTL002

*2Only the COM port which can communicate by RS-232C can be used.

IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.