### MELSEC L Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Input Relay | X0000-X1FFF | X0000-X1FF0 |  |
Output Relay | Y0000-Y1FFF | Y0000-Y1FF0 |
Internal Relay | M00000-M61439 | M00000-M61424 |
Special Relay | SM0000-SM2047 | SM0000-SM2032 |
Latch Relay | L00000-L32767 | L00000-L32752 |
Annunciator | F0000-F32767 | F00000-F32752 |
Edge Relay | V00000-V32767 | V00000-V32752 |
Step Relay | S0000-S8191 | S0000-S8176 |
Link Relay | B0000-BEFFF | B0000-BEFF0 |
Special Link Relay | SB0000-SB7FFF | SB0000-SB7FF0 |
Timer (Contact) | TS00000-TS25471 | ------ |
Timer (Coil) | TC00000-TC25471 | ------ |
Retentive Timer (Contact) | SS00000-SS25471 | ------ |
Retentive Timer (Coil) | SC00000-SC25471 | ------ |
Counter (Contact) | CS00000-CS25471 | ------ |
Counter (Coil) | CC00000-CC25471 | ------ |
Timer (Current Value) | ------ | TN00000-TN25471 |
Retentive Timer (Current Value) | ------ | SN00000-SN25471 |
Counter (Current Value) | ------ | CN00000-CN25471 |
Data Register | ------ | D00000-D65535 |
Special Register | ------ | SD0000-SD2047 |
Link Register | ------ | W0000-WFFFF |
Special Link Register | ------ | SW0000-SW6FFF |
Module Access Device | ------ | U000-G00000-U1FF-G65535 | *2
File Register (Normal) | ------ | R00000-R32767 | *1
File Register (Block switching is not necessary) | ------ | ZR0000000-ZR393215 | *1
File Register (0R - 11R) | ------ | 0R00000-0R32767 | *1
------ | 1R00000-1R32767
------ | 2R00000-2R32767
: | :
------ | 10R00000-10R32767
------ | 11R00000-11R32767

*1It is different by the memory card which uses the range of file register.

*2This device enables access of the Buffer Memory of SLMP compatible devices or Intelligent Function Modules. The first 3 digits in the address field specify the start I/O number of the intelligent module.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms