### Settings of External Device

Use the ladder software "PL7 PRO" for communication settings.

Double-click "Hardware Configuration" from "Configuration" in "Application Browser" of "PL7 PRO". Next, double-click "Comm" in the "Configuration" dialog box. Perform the settings in the displayed dialog box.

Setup Items | Setup Description
--- | ---
CHANNEL | CHANNEL 1
TSX SCP 111 RS232 MP PCMCIA CARD
MODBUS/JBUS LINK | MAST
Type | Slave
Slave number | 1
Transmission speed | 9600bps
Delay between characters | 4msec
Data | RTU (8 bit)
Stop | 1 bit
Parity | Even

NOTE

- Please refer to the manual of the ladder software for more detail on other setting description.

- Use an integer from 1 to 247 to enter the unit ID of the External Device.