### Setting of External Device

Select [PLC System Register Setting] from [Option] of the tool bar in the ladder software to display the [PLC System Register Setting] dialog box. Select the [COM1(2) Port Setting] tab to set as below. Please refer to the manual of the External Device for more details.

Setup Items | Setting Value
--- | ---
Speed | 19200
Data Length | 8
Parity | Odd
Stop Bit | 1
Communication Mode | Computer link
Modem Connection | OFF
Unit No. | 1

* For COM1 of AFPG806, you need to set the built-in switch on the rear of the cassette.

DIP Switch | Settings | Setup Description
SW1-2 | OFF | Line Speed