### PXR (AutoFIX) / PXR (NoAutoFIX) series

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Bit Data | 00001 | - |  | *1
Read Only Bit Data | 10001 - 10016 | 10001 | *2
Read Only Word Data (Internal) | - | 30001 - 30037 | *2
Read Only Word Data (Engineering Unit) | - | 31001 - 31037 | *2
Word Data (Internal) | 40001.00 - 40120.15 | 40001 - 40120 | *1 *3
Word Data (Engineering Unit) | 41001.00 - 41120.15 | 41001 - 41120 | *1 *3

*100001, 40001, and 41001 are addresses to order writing in the nonvolatile memory (FIX processing).
Writing in the nonvolatile memory is performed by entering 1 (one) to the writing value.

*2Write disabled.

*3When you write to the bit address, the Display reads the entire word, sets the defined bit, then returns the new word value to the External Device. If the ladder program writes data to this word address during the bit write process, the resulting data may be incorrect.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms