### 8B)

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) External Device side: D-Sub 9 pin (socket) | Instead of connecting the Display (FG), connect the Shield to the Shell.
(2) | Communication adapter by Mitsubishi Electric Corp. FX3U-232ADP or FX3U-232ADP-MB |
(3) | Function extension board by Mitsubishi Electric Corp. FX3U-232-BD, FX3U-422-BD, FX3U-485-BD, FX3U-USB-BD, FX3U-CNV-BD, FX3G-CNV-ADP or FX3S-CNV-ADP |