### TC200S series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Input Relay 1 | X000 - XF7F | X00W - XF7W |  | *1
Input Relay 2 | I000 - IF7F | I00W - IF7W | *1
Output Relay 1 | Y000 - YF7F | Y00W - YF7W | *1
Output Relay 2 | O000 - OF7F | O00W - OF7W | *1
Internal Relay | R000 - R77F | R00W - R77W | *1
Extended Internal Relay 1 | G000 - GF7F | G00W - GF7W | *1
Extended Internal Relay 2 | H000 - HF7F | H00W - HF7W | *1
Extended Internal Relay 3 | J000 - JF7F | J00W - JF7W | *1
Extended Internal Relay 4 | K000 - KF7F | K00W - KF7W | *1
Special AUX Relay | A000 - A16F | A00W - A16W | *1
Latch Relay | L000 - L07F | L00W - L07W | *1
Shift Register | S000 - S07F | S00W - S07W | *1
Edge Relay | E000 - E77F | E00W - E77W | *1
Timer (contact) | T000 - T77F | T00W - T77W | *1 *2
Counter (contact) | C000 - C77F | C00W - C77W | *1 *3
Timer/Counter (current value) | ------ | P000 - P77F | *1
Timer/Counter (setup value) | ------ | V000 - V77F | *1
Generic Register 1 | ------ | D000 - DF7F | *1
Generic Register 2 | ------ | B000 - BF7F | *1
Generic Register 3 | ------ | U000 - UF7F | *1
Generic Register 4 | ------ | M000 - MF7F | *1
Generic Register 5 | ------ | Q000 - QF7F | *1

*1Device format is as follows: Please refer to the manual of External Device for more detail. *2The addresses of the timer (contact) range from T00W to T77W, however the internal memory area is not consecutive. This range is divided into two areas, e.g., T00W to T37W and T40W to T77W. *3The addresses of the counter (contact) range from C00W to C77W, however the internal memory area is not consecutive. This range is divided into two areas, e.g., C00W to C37W and C40W to C77W.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms