# Equipment

Property | Description | Data Type | Minimum Value | Maximum Value | Read | Write | Retentive
ErrorFlag | When there is a communication error, this flag is set True. Manually reset the flag after confirming the error. | BOOL | - | - |  |  | -
ErrorStatus | The communication error status is set. 0: No error 1: Error 2: Not in use (When communication scan is turned off.) If the communication recovers, 0 is set to the [ErrorStatus] after the deadband period has passed. From the [Equipment] property window, configure the deadband interval in [Error Status Deadband (seconds)] | Integer | - | - |  | - | -
IPAddress.CurrentValue*2 | Current IP address of equipment. | DWORD | 1 | 4294967295 |  | - |
IPAddress.OverWriteValue*2 | IP address that you want to set to equipment. This value is applied to the associated equipment’s IP address when save is performed in a script using the [Equipment] operation. Equipment | DWORD | 1 | 4294967295 |  |  | -
ScanOffStatus*1 | Current equipment communication scan status. True: Communication scan is stopped. False: Communication scan of equipment is running. Note: When an equipment’s communication scan is turned off, the quality of variables associated with the equipment will be “bad” and objects using the variables will display a red border to indicate a communication error. If a block script uses a variable with bad quality, the block script is skipped. For operation of a block script that uses a variable with bad quality, refer to the following. Types of Blocks | BOOL | - | - |  | - | -
ScanOffControl*1 | Turns communication scans of the equipment on or off, without requiring save and restart. False: Turn communication scan on. True: Turn communication scan off. | BOOL | - | - |  |  |
UnitId.CurrentValue*2 | Displays the current unit ID. (Modbus SIO Master driver / Modbus SIO ASCII Master driver) | UINT | 1 | 247 |  | - |
Displays the current unit ID. (Modbus TCP Master driver) | UNIT | 0 | 255 |  | - |
UnitId.OverWriteValue*2 | Set the unit ID that you want for the equipment. This value is applied to the associated equipment’s unit ID when save is performed in a script using the [Equipment] operation. (Modbus SIO Master driver / Modbus SIO ASCII Master driver) Equipment | UNIT | 1 | 247 |  |  | -
Set the unit ID that you want for the equipment. This value is applied to the associated equipment’s unit ID when save is performed in a script using the [Equipment] operation. (Modbus TCP Master driver) Equipment | UNIT | 0 | 255 |  |  | -

*1 Source property is NOT supported by equipment for the following drivers:

- Modbus Organization

- Modbus SIO Slave
- Modbus TCP Slave

- Pro-face by Schneider Electric

- Memory Link Ethernet
- Memory Link SIO

- Schneider Electric

- EcoStruxure Augmented Operator Advisor

*2 Source property is supported by equipment for the following drivers:

- Modbus Organization

- Modbus SIO ASCII Master
- Modbus SIO Master

- Modbus TCP Master

- Schneider Electric

- Modbus SIO Master

- Modbus TCP Master